W2W Coast Station Server

MF/HF Transmitter

YaDDNet DSC Database

UDP/IP Message feed from YaDDNet to W2W Coast Station Server

Admin / Monitor PC

USB Connection:

Audio and Transmitter control

TCP/IP connection for admin

UDP/IP and TCP/IP connections to YaDDNet from multiple receivers .

UDP/IP message feed from YaDD v1.7

